|  |
| --- |
| CAE simulation 5 |

**Date : 2023.10.26**

**ID : 21800773**

**Subject : ansys analysis of coal compression equipment**

**Name : HanMinwoong**

**1. Problem**

We are trying to manufacture a coal compression equipment. (Material SS400) The hydraulic jockey placed on the lower beam can apply a force of up to 12 tons to the molding cylinderplaced on the center beam. Currently, the molded cylinder is in contact with the upper beam and the upper beam is loaded, and raw coal is squeezed inside the cylinder to manufacture the formed coal. The hydraulic jack is placed on the lower beam. A 1/4 CAD model is used for simulation considering the geometric symmetry.

**2. Simulation result**

**텍스트, 스크린샷, 디자인이(가) 표시된 사진

자동 생성된 설명**

**Figure 1. Stress analysis of quarter model**

**2.1. Full model**

|  |  |
| --- | --- |
| **Mesh size =** | **Mesh size =** |
|  |  |
| **Mesh size =** | **Mesh size = 2** |
|  |  |

**텍스트, 스크린샷, 도표, 그래프이(가) 표시된 사진

자동 생성된 설명**

**Figure 2. Mesh convergence**

As can be seen in the **Figure 2**, mesh equivalent stress converges as mesh size decreases.